**To,**

**Courtyard Marriott,**

**Teynampet, Chennai.**

**Ref.: CEPL/2020-21/085,**

**Date: 16th February 2021,**

**Dear Sir,**

**Sub: Application of Dr Fixit Rain Coat WPC and Repair Work – Reg.**

We refer to the above.

Subsequent to the discussion and Site Visit, We are pleased to submit the quotation for Application of Dr. Fixit Rain Coat WPC as per specifications enclosed.

Please do not hesitate to contact us for any further clarifications.

Assuring you of our best service and attentions at times. Look forward to receive your order at the earliest.

Thanking you,

Yours faithfully,

**For CIVITECH ENGINEERING PRIVATE LTD,**

**Mr. Subishwar Murali**

**EXECUTIVE DIRECTOR.**

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **External Wall Waterproofing With Dr. Fixit Raincoat WPC & Raincoat Classic System** | | | | | |
| **STAGE** | **ITEM DESCRIPTION** | **UNIT** | **QTY** | **RATE** | **TOTAL** |
| SURFACE PREPARATION |  | Sqm | 10500 | 98.50 | 10,34,250.00 |
| Cleaning and preparation of surface with the help of wire brush & washing down the external wall and remove all loose mortar and laitance, etc., and washing with plenty of water |
|
| All hairline should be opened to atleast 1 to 5 mm with “undercut” groove for ease of application, then filled with acrylic crack filler Dr. Fixit Cracks-X paste of M/s Pidilite Industries Ltd. Grouting the water outlet gaps space between the slab & parapet wall with non- shrink grout Dr. Fixit Pidigrout 10M or by preparing cement polymer modified mortar with Dr. Fixit Pidicrete URP in the ratio of 1:3 by adding polymer 10% by weight of the cement. |
| Providing, mixing and applying single coat of penetrating acrylic waterproof Primer **Dr. Fixit Primeseal** dilute with water in the ratio 2:1 spreading at the rate of 8-10 /Sq.mt /Litre Substrate MUST be in SSD condition for application of primer. |
|
| APPLICATION | Providing & Applying first coat of **Dr. Fixit Raincoat Waterproof Coating(WPC)** without any dilution. Maintain the spreading rate of 4.20 - 4.70 sq mtr per litre / coat application to achieve about 100-120 microns DFT. Providing & Applying second coat of **Dr. Fixit Raincoat Classic** Top coat with interval of 6-8 hours without any dilutionone coats of Dr. Fixit Raincoat Waterproof Coating without any dilution by maintaining spreading rate of 6.0 -6.5 sq mtr / per litre / coat to achieve 50 –60 microns DFT. Achieving total DFT of 160 to 180 microns. The material having following technical properties: Attains hairline crack bridging up to 2 mm, Elongation of >100 % as and Tensile 2.50 Mpa per ASTM D 412. | Sqm | 10500 | 283.75 | 29,79,375.00 |
|

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Structural Repair with Dr Fixit Pidicreate URP (Polymer Plastering)** | | | | | |
| **STAGE** | **ITEM DESCRIPTION** | **UNIT** | **QTY** | **RATE** | **TOTAL** |
| SURFACE PREPARATION |  | Sqm Approx | 100 | 750.00 | 75,000.00 |
| Chipping the loose portion of the existing column. Clean the surface and make sure that surface is clean and free from loose particle. |
|
| Supply and application of **Z**inc Rich Primer**,** one/two component, zinc rich, epoxy primer shall be brush applied to the exposed rebars all around in two coats and allowed to fully dry. |
| Providing and applying Dr Fixit Epoxy Bonding Agent, two component epoxy resin bonding agent over the prepared concrete surface and allowed to achieve tacky condition. |
|
| APPLICATION | Provide and apply Polymer Plastering on the bonding agent applied surfaces while in tacky condition. Providing and Applying Polymer modified morter in C.M 1:3 admixed with Pidicrete URP @ 2 Ltrs per bag of cement and applyed in average thickness of 50mm using steel trowel. | Sqm Approx | 100 | 1,600.00 | 1,60,000.00 |
|
| SCAFFOLDING CHARGES | Providing and fixing of scaffolding to external side of building. Rate inclisve of trasnporation, shiffing and fixing. | Sqm Approx | 300 | 200.00 | 60,000.00 |
|
| Charges for removing and refixing of scaffolding including labour and shiffing charges. | Sqm Approx | 300 | 100.00 | 30,000.00 |

**TERMS AND CONDITIONS**

1. Work shall be commenced immediate on receipt of your order confirmation along with advance payment.
2. **Payment:** We require 50% of order value as advance along with the order and the balance payment against running bills.
3. GST shall be 18% Extra.
4. The Client shall provide Clean water confirming to **IS 456-2000** and electricity required for the treatment at free of cost.
5. **Godown**  facility for storing our materials shall be provided by the client.
6. Measurement shall be on actual area treated.