**Hyundai Motors India Pvt Ltd**

**Sriperambathur,**

**Chennai’**

**Ref.: CEPL: Qtn: 10:2020:27,**

**Date: 30th October 2020**

Dear Sir,

**Sub: Quote for Epoxy floor coating: - Reg.**

**Ref: Your enquiry with us.**

We refer to the discussion the undersigned had with you.

As requested, we are pleased to submit our quote for supply and application of Epoxy Floor coating system with 3mm.

Hope our offer is in line with your requirement and looking forward to receive your valued order confirmation.

In the meantime, assuring you of our best services and attention at all times.

Thanking you,

Yours faithfully,

**For CIVITECH ENGG. PVT. LTD.,**

# MRS MURALI

 **DIRECTOR.**

.

# APPLICATION PROCEDURE FOR FLOORING

***SURFACE PREPARATION:***

Surface shall be prepared by mile scarification using scarifier to get mechanical key effect to the primer and the concrete surface for ensuring maximum bonding. Dust and loose particles shall be cleaned using vacuum cleaners. Neither water wash nor acid etching should be used for cleaning.

**Application Of Primer**

Make sure the surface is bone dry during application of primer NITOPRIME 25(M). The two part system shall be mixed mechanically using a slow speed heavy duty drilling machine (400 to 500 rpm) fitted with a suitable paddle to achieve homogeneous mix and shall be applied on the prepared surface. Coverage should not exceed 35 Sq.m./Pack.

**Base Layer**

**Fosroc Nitoflor SL**, a high strength self smoothing epoxy underlay is applied as the base layer. The base, hardener and filler components of **Fosroc Nitoflor SL** shall be mixed thoroughly until getting a homogeneous mix and the same be poured on to the prepared surface and spread evenly to maintain the required thickness using a serrated trowel followed by that spike roller shall be rolled over the leveled underlay to remove any entrapped air and allowed to cure for a day.

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| S.NO |  DESCRIPTION | **Unit** | **Qty.** | Rate |  |
| **01.** | Supply and Application of Epoxy systems using Fosrcoc Nitoflor SL covering the following sequence of operation:Providing and laying epoxy floor coating system over the prepared surface, Applying **Fosroc** **Nitoflor SL** .. Quoted rate is inclusive of surface preparation, chemicals and application charges  **2mm** **3mm**GST Tax @18% Extra | sft |  | **140.00** |  |

##### TERMS AND CONDITIONS

1. Work shall be commenced on receipt of your work order.
2. **Payment:** 70 % of order value shall be paid as advance, balance payment after completion of work.
3. The client at shall provide water and electricity required for the treatment free of cost.